{"text_format":"2","workbook":"xls","n_sheets":5,"sheets":["Radials","Storleksordn","Sheet2","In-lines","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Radials","index":0,"n_rows":79,"n_cols":19,"rows_kept":79,"cut":false,"hidden":false,"merged":[[0,14,0,15],[0,0,0,12]],"flags":["formulas_cached_only"]}
["Motor",{"$nulls":12},"Plan","Pris utomlands",null,"HAB"]
["Fabr","Typ","Bränsle","cyl","cc","hp","kg","dia ","längd","prop","rpm","drag","bränsle","kg","var","pris i kr ","pris","anm"]
[{"$nulls":7},"mm","mm",null,null,"kp","förbr"]
[{"$nulls":12},"cc/min"]
["SAITO","FA 90 R3","Met+20%N",3,15.1,0.95,0.85,156,129,"12/13",8500,3,25,null,"Horizon",5600,6400]
["SAITO","FA 120 R3","Met+20%N",3,19.2,null,0.9,168,129,"13/14",10000,3.5,25]
["SAITO","FA 170 R3","Met+20%N",3,28,2.5,1.3,186,155,"15/16",null,6.3,45,null,"Horizon",6650,8000]
["SAITO","FA 200 R3","Met+20%N",3,33,2.7,1.38,186,155,"16/17",9500,10,46]
["SAITO","FA 325 R5D","Met+20%N",5,53,3.8,2.4,220,170,"20x10",7500,12,75,null,"Horizon",14000,17500]
["SAITO","FA 450 R3D","Met+20%N",3,73,5.5,2.8,237,200,"21/24",7000,21,60,null,"Horizon",10500,12800]
[]
["OS","FR5-300Sirius","Metanol",5,49,4,2.7,234,160,"18/22",null,12,null,null,"HAB",21460,null,"rpm 8500, tot längd till prop 160mm"]
["OS","FR7-420Sirius","Metanol",7,70,null,3.2,230,160,null,7000,20]
[{"$nulls":17},"13650:- rcplanet"]
["ROBART","R 780","Metanol",7,128,10,3.8,250,null,"24x8",{"$nulls":4},"Robart",28000]
[]
["SL Engines",null,"Bensin",7,90,10,3.8,240,null,"30x8",7500,null,null,null,"MOKI Italia",25600]
["SL Engines",null,"Metanol",7,null,null,3.2,240,null,"26/28"]
[]
["MOKI","RCS 150","Bensin",5,150,8.5,4.5,255,215,"28/30",{"$nulls":4},"Troybuilt mod",22400]
["MOKI","RCS 180","Bensin",5,180,9.5,4.6,265,215,"28/30"]
["MOKI","RCS 215","Bensin",5,215,13.5,5.5,285,205,40,5200,null,null,null,"Troybuilt mod",25200]
["MOKI","RCS 250","Bensin",5,250,15,5.4,285,205,"32/34",{"$nulls":4},"Troybuilt mod",28000]
["MOKI","RCS 250","Bensin",7,250,15.5,5.5,295,205,32]
["MOKI","RCS 400","Bensin",5,400,25,9.2,350,260,40,3800,null,null,null,"Troybuilt mod",40600]
[]
["Techno pwr","A series","Met, 15% N",7,22,0.75,0.9,152,78,14,7500,3.5,null,3.6,"Technopower",17500,null,"10% olja, 15% N"]
["Techno pwr","B series","Met, 15% N",7,32,1,0.9,168,78,"14/16",7500,6.3,null,5.5,"Technopower",17500]
["Techno pwr","B series","Met, 15% N",9,41,1.6,1.2,180,83,"16/20",7500,12,null,7.3,"Technopower",19300]
["Techno pwr","C series","Met, 15% N",9,67,2.5,2.1,225,98,"18/24",7500,20,null,10,"Technopower",20300]
[]
["Seidel","ST-7-35","Met ??",7,35,2,1.4,187,153,"2018-06-08",5200,null,null,null,"Seidel"]
["Seidel","ST-7-70","Met, 15% N",7,70,4,2.6,230,null,"24/26",{"$nulls":4},"Seidel",10200,12100,"Spv 2,2m  tot-vikt  14 kg max"]
["Seidel","ST-9-90","Met, 15% N",9,90,5.4,3.5,260,null,"30/38",{"$nulls":4},"Seidel",15300,17000,"Dito"]
["Seidel","ST-7-160","Bensin",7,160,10,4.3,260,null,"38/40",{"$nulls":4},"Seidel",20500,24000,"2,6m       20kg"]
["Seidel","ST-7-250","Bensin",7,250,14,6,315,null,"40/42",{"$nulls":4},"Seidel",24600,28000,"3 - 4m       30kg"]
["Seidel","ST-14-500","Bensin",14,500,22,12,320,null,"40x20",{"$nulls":4},"Seidel","-",null,"4 - 4,5m       40kg"]
["Seidel","ST-7-700","Bensin",7,700,40,15,440,null,"40/42",{"$nulls":4},"Seidel","-"]
[]
["Seidel UMS","ST-7-35","Met, 15% N",7,35,2,1.3,187,153,"16/20",5200,null,null,null,"UMS",9200]
["Seidel UMS","ST-7-70","Met, 15% N",7,70,4,2.6,235,198,"24/26",6300,null,null,null,"UMS",10000,null,null,1.4]
["Seidel UMS","ST-9-90","Met, 15% N",9,90,5.4,3.5,262,198,"26/28",6000,null,null,null,"UMS",14600]
["Seidel UMS","ST-7-250","Bensin",7,250,14,6,332,272,"32/38",5500,null,null,null,"UMS",24400]
[]
["Magnum,","XL 400-5R","Met, + N",5,64,7.5,2.8,220,200,"18/22",9000,null,null,null,"Hi-model",6100,null," brusten clipskant vevstakspinne"]
["ASP, SC","FS 400 AR",{"$nulls":12},"HAB",10000,null,"prop 22x8  6500rpm/24x12 5000 rpm"]
[]
["Valach Eng.","VM R5-420","Bensin",5,420,null,12,425,255,"38/42",4500,null,null,60,"Valach",40000]
["Valach Eng.","VM R7-800","Bensin",7,800,null,28,550,300,"48/52",3800,null,null,70,"Valach",70000]
["Valach Eng.","VM R9-1250","Bensin",9,1250,null,37,null,null,null,3000]
[]
["Auth scale","R 5-50 M","Met+20%O",5,57,{"$nulls":12},"coming soon"]
[null,"R 9-90 M","Met+20%O",9,90,null,4,240,190,"24/27",5000]
[null,"R 14-100 M","Met+20%O",14,97,null,4.4,235,"195?","24/28",5000]
[]
["Evolution"," E 7-35","Met+7%olja",7,35,1.8,1.4,185,160,"16/18",5200,6]
["Evolution"," E 7-77","Met+7%olja",7,77,4.8,2.6,230,200,24,6000]
["Evolution"," E 9-99","Met+7%olja",9,99,6.9,3.5,260,200,"26/28",6500]
["Evolution"," E 7-160","Bensin 32:1",7,160,10.6,4.8,290,180,"27/28",6000,{"$nulls":6},"2900 USD"]
["Evolution"," E 7-260","Bensin 32:1",7,260,15.6,6.7,330,206,"30/32",5800,{"$nulls":6},"3400 USD"]
[]
["Ohrndorf",null,"Met+20%O",9,90,null,4,250,140,"26/2bl-24/3bl",5000,null,null,null,"Klass Kote",22000]
[null,null,"Met+20%O",14,97,null,4.3,235,195,"28/2bl-26/3bl",4500]
[]
["Brownbear","Penta 54","M+7%O+5%N",5,54,null,2.9,221,145,"20/22",7000]
["Brownbear","Penta 85","M+7%O+5%N",5,85,null,3.9,260,155,"24/26",5300]
["Brownbear","Penta 102","M+7%O+5%N",5,102,null,4,260,155,"26/28",5200]
["Brownbear","Septa 120","M+7%O+5%N",7,120,null,4.8,271,165,"28/29",5000]
["Brownbear","Septa 162","M+7%O+5%N",7,162,null,5.2,288,168,"29/30",4800]
{"$rows_empty":9}
[{"$nulls":15},"ORC"]

{"sheet":"Storleksordn","index":1,"n_rows":42,"n_cols":16,"rows_kept":42,"cut":false,"hidden":false,"merged":[[0,0,0,10],[0,12,0,13]],"flags":["formulas_cached_only"]}
["Motor",{"$nulls":10},"Plan","Pris utomlands",null,"HAB"]
["Fabr","Typ","Bränsle","cyl","cc","hp","kg","dia ","längd","prop","rpm","kg","var","pris i kr ","pris","anm"]
["SAITO","FA 90 R3","Met+20%N",3,15.1,0.95,0.9,168,null,"12/13",null,null,"Horizon",5600,6400]
["Techno pwr","A series","Met, 15% N",7,22,0.75,0.9,152,null,14,7500,3.6,"Technopower",17500,null,"10% olja, 15% N"]
["SAITO","FA 170 R3","Met+20%N",3,28,2,1.3,200,null,"15/16",null,null,"Horizon",6650,8000]
["Techno pwr","B series","Met, 15% N",7,32,1,0.9,168,null,"14/16",7500,5.5,"Technopower",17500]
["Seidel UMS","ST-7-35","Met, 15% N",7,35,2,1.3,187,153,"16/20",5200,null,"UMS",9200]
["Techno pwr","B series","Met, 15% N",9,41,1.6,1.2,180,null,"16/20",7500,7.3,"Technopower",19300]
["OS","FR5-300Sirius","Metanol",5,49,4,2.7,234,null,"18/22",null,null,"HAB",21460,null,"rpm 8500, tot längd till prop 160mm"]
["SAITO","FA 325 R5D","Met+20%N",5,53,3.8,2.4,220,null,"20x10",null,null,"Horizon",14000,17500]
["Magnum,","XL 400-5R","Met, + N",5,64,7.5,2.8,220,160,"18/22",6500,null,"Hi-model",6100,null," brusten clipskant vevstakspinne"]
["Techno pwr","C series","Met, 15% N",9,67,2.5,2.1,225,null,"18/24",7500,10,"Technopower",20300]
["Seidel","ST-7-70","Met, 15% N",7,70,4,2.6,230,null,"24/26",null,null,"Seidel",10200,12100,"Spv 2,2m  tot-vikt  14 kg max"]
["Seidel UMS","ST-7-70","Met, 15% N",7,70,4,2.6,235,198,"24/26",6300,null,"UMS",10000]
["SAITO","FA 450 R3D","Met+20%N",3,73,5.5,3,250,null,"21/24",null,null,"Horizon",10500,12800]
["SL Engines",null,"Bensin",7,90,10,3.8,240,null,"30x8",7500,null,"MOKI Italia",25600]
["Seidel","ST-9-90","Met, 15% N",9,90,5.4,3.5,260,null,"30/38",null,null,"Seidel",15300,17000,"Dito"]
["Seidel UMS","ST-9-90","Met, 15% N",9,90,5.4,3.5,262,198,"26/28",6000,null,"UMS",14600]
["ROBART","R 780","Metanol",7,128,10,3.8,250,null,"24x8",null,null,"Robart",28000]
["MOKI","RCS 150","Bensin",5,150,8.5,4.5,255,null,"28/30",null,null,"Troybuilt mod",22400]
["Seidel","ST-7-160","Bensin",7,160,10,4.3,260,null,"38/40",null,null,"Seidel",20500,24000,"2,6m       20kg"]
["MOKI","RCS 215","Bensin",5,215,13.5,5.5,285,null,40,5200,null,"Troybuilt mod",25200]
["MOKI","RCS 250","Bensin",5,250,15,5.4,285,null,"32/34",null,null,"Troybuilt mod",28000]
["Seidel","ST-7-250","Bensin",7,250,14,6,315,null,"40/42",null,null,"Seidel",24600,28000,"3 - 4m       30kg"]
["Seidel UMS","ST-7-250","Bensin",7,250,14,6,332,272,"32/38",5500,null,"UMS",24400]
["MOKI","RCS 400","Bensin",5,400,25,9.2,350,null,40,3800,null,"Troybuilt mod",40600]
["Valach Eng.","VM R5-420","Bensin",5,420,null,12,425,255,"38/42",4500,60,"Valach",40000]
["Seidel","ST-14-500","Bensin",14,500,22,12,320,null,"40x20",null,null,"Seidel","-",null,"4 - 4,5m       40kg"]
["Seidel","ST-7-700","Bensin",7,700,40,15,440,null,"40/42",null,null,"Seidel","-"]
["Valach Eng.","VM R7-800","Bensin",7,800,null,28,550,300,"48/52",3800,70,"Valach",70000]
["Fabr","Typ","Bränsle","cyl","cc","hp","kg","dia ","längd","prop","rpm","kg","var","pris i kr ","pris","anm"]
[{"$nulls":7},"mm","mm"]
[]
[{"$nulls":15},"13650:- rcplanet"]
[]
["SL Engines",null,"Metanol",7,null,null,3.2,240,null,"26/28"]
[]
[]
[]
[]
[]
["ASP, SC","FT 400 AR",{"$nulls":10},"HAB",10000,null,"prop 22x8  6500rpm/24x12 5000 rpm"]

{"sheet":"Sheet2","index":2,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Fabrikat","Typ","Bränsle","cyl","cc"]
[]
["SAITO","E 90","Met, + N",3,15]
["SAITO","FA 170 R3","Met, + N",3,28]
["SAITO","FA 325 R5D","Met, + N",5,53]
["SAITO","FA 450 R3D","Met, + N",3,73]
[]
["OS","FR5-300Sirius","Met, + N",5,49]
[]
["ROBART","R 780","Met, + N",7,128]
[]
["SL Engines",null,"Met, + N",7,90]
["SL Engines",null,"Bensin",7,90]
[]
["MOKI","RCS 150","Bensin",5,150]
["MOKI","RCS 215","Bensin",5,215]
["MOKI","RCS 250","Bensin",5,250]
["MOKI","RCS 400","Bensin",5,400]
[]
["Techno pwr","A series","Met, + N",7,22]
["Techno pwr","B series","Met, + N",7,32]
["Techno pwr","B series","Met, + N",9,41]
["Techno pwr","C series","Met, + N",9,67]
[]
["Magnum","XL 400-5R","Met, + N",5,64]
["ASP","Dito"]
["SC","Dito"]
["DC","Dito"]

{"sheet":"In-lines","index":3,"n_rows":18,"n_cols":16,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,0,0,10],[0,12,0,13]],"flags":["formulas_cached_only"]}
["Motor",{"$nulls":10},"Plan","Pris utomlands",null,"HAB"]
["Fabr","Typ","Bränsle","cyl","cc","kW","kg","bredd","längd","prop","rpm","kg","var","pris i kr ","pris","anm"]
[]
["Brownbear","In line Qadrup","M+7%O+5%N",4,130,null,5,null,278,"29x12",5100]
[]
["Kolm","IL 100    4 Takt","Bensin 1:50",2,100,null,3]
["Kolm","IL 130","Bensin 1:50",2,135,8.8,3.7,123,255,"28/30",5500,null,null,24000]
[]
["OS","IL 300    4 Takt","M+20%olja+N",4,50,null,2.3,80,234,"20/22",8000]
[]
["MOKI","M 360  2 Takt","M+20%olja+N",2,60,5.7,2.3,80,195,"22/24",12000]
[null,"G 360","Bensin 1:50",2,60,5.4,2.5,100,234,24,11000]
[]
["SAITO","FA-100 Ti 4 Takt","M+20%olja+N",2,18,null,1.1,76,149,"14/15",10000]
["SAITO","FA-200 Ti","M+20%olja+N",2,33,null,1.5,110,160,"16/18",9200]
[]
["ZDZ","100 R2  2Takt","Bensin 1:40",2,97,null,2.8,null,248,"24/27",8200]
["ZDZ","150 R3    2 Takt","Bensin 1:40",3,150,null,2.8,null,329,"28/30",8200,null,null,13000]

{"sheet":"Sheet3","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}